The Dialog Customer Server will be stared when the startup your computer.

After the startup your computer it will search the GSM 900 modem port and connect to the Dialog SQL Server.

If both tracks are completed, the Dialog Customer Server sends SMS to the Sever Administrator of the Computer.

Once, the sending SMS is completed, it is ready to used and waiting for customer SMS.

When a customer send SMS to the Server in a correct format, the dialog Customer Server will revised the SMS and upload to the SQL Server.

*"Message Server GSM SIM 800A COM Port Warning"*

*"Check the com port and try again. The message server serial port can't be opened."*

If this error message is appeared, you need to check your GSM 900 Modem is plug in to USB port. Although, the GSM 900 Modem is plug in to USB port and If this error message is still appeared, Then you need to unplug GSM 900 Modem from the USB port, plug it again.